# Release Notes for MT25TL01G QuadSPI Component Driver

Copyright © 2016 STMicroelectronics

# License

This software component is licensed by ST under BSD 3-Clause license, the “License”; You may not use this component except in compliance with the License. You may obtain a copy of the License at: https://opensource.org/licenses/BSD-3-Clause

# Purpose

This driver provides a set of QuadSPI functions offered by MT25TL01G component

# Update History

V2.3.0 / 02-Febraury-2021

## Main Changes

- Update MT25TL01G_DIE_ERASE_CMD value

##

V2.2.0 / 29-January-2021

## Main Changes

- Fix MT25TL01G_ReadStatusRegister to use MT25TL01G_READ_STATUS_REG_CMD command instead of MT25TL01G_READ_FLAG_STATUS_REG_CMD

##

V2.1.0 / 24-Febraury-2020

## Main Changes

- Set right data length for SPI mode

##

V2.0.0 / 23-November-2019

## Main Changes

- First Official release of MT25TL01G BSP drivers in line with STM32Cube BSP drivers development guidelines (UM2298)
- The component drivers are composed of
  - component core drivers files: mt25tl01g.h/.c
  - component configuration files: mt25tl01g_conf_template.h

## Backward Compatibility

- This version breaks the compatibility with previous versions

##

V1.0.0 / 08-August-2016

## Main Changes

- First official release of MT25TL01G QuadSPI driver

##