# Release Notes for OV9655 Component Driver

Copyright © 2019 STMicroelectronics

# License

This software component is licensed by ST under BSD 3-Clause license, the “License”; You may not use this component except in compliance with the License. You may obtain a copy of the License at:
https://opensource.org/licenses/BSD-3-Clause

# Purpose

This driver provides a set of camera functions offered by OV9655 component

# Update History

V2.2.0 / 15-December-2020

## Main Changes

- Fix Mirror/Flip setting in OV9655_MirrorFlipConfig API:
  - Clear Bit[4:5] corresponding to mirror/flip selection before applaying the new configuration

## Backward Compatibility

- None

## Dependencies

This software release is compatible with:

- BSP Common v6.0.0 or above

V2.1.0 / 30-September-2020

## Main Changes

- Fix pixel format setting in OV9655_SetPixelFormat API:
  - Clear Bit[0:1] corresponding to pixel format selection before applaying the new configuration
  - Update registers TSLB and COMMON15 required for setting YUV format

## Backward Compatibility

- None

## Dependencies

This software release is compatible with:

- BSP Common v6.0.0 or above

V2.0.0 / 30-October-2019

## Main Changes

- First Official Release version of OV9655 Camera sensor Component in line with STM32Cube BSP drivers development guidelines (UM2298)
- The component drivers are composed of
  - component core drivers files: ov9655.h/.c
  - component register drivers files: ov9655_regs.h/.c

## Backward Compatibility

This version breaks the compatibility with previous versions

## Dependencies

This software release is compatible with:

- BSP Common v6.0.0 or above

V1.0.1 / 07-April-2017

## Main Changes

- Update comments to be used for PDSC generation

V1.0.0 / 25-June-2015

## Main Changes

- First official release of OV9655 Camera sensor driver